Waterproof connector for 3 wires. 30009947

Details:


* The unique "U" contact provides a reliable electrical connection up to 600 V.
* Quick and easy to use, simply click shut without stripping or twisting the wire
* UL Listed, VDE Certified, IEC 60998-3-2 Tested
* Moisture resistant in wet environments when used with distribution box.
* Humid environmental applications (moisture resistant)

This connector is used in Fri-Jado appliances with moist environments.

Take following steps and use accordingly.


Step1. Do not strip the wire

Good Not Good


 

Step 2. Push wire until end of connector

Good Not Good


 

Not Good

Step 3.


Push all three wires until the end of the connector, as shown below.

Wire ends must be visible



Step 4.

Using a pipe wrench, push the blue cap into the connector.



Make sure the cap is pushed entirely into the connector.

Good Not Good

Final Check:

* Wire ends are visible , and reaching the end of the connector (top)
* Blue cap is pushed completely into the connector.

